# Polystyrene Sulfonic Acid (PSSA)

|  |  |  |
| --- | --- | --- |
| Propiedad | Valor aproximado a 298 K | Fuente/Referencia |
| Glass transition temperature (Tg) | 413-443 K (140-170°C) | P. Cebe et al., Macromolecules (1982) |
| Solubility in water | Soluble | A. Eisenberg, Macromolecules (1970) |
| Heat capacity | 1.4-1.6 J/g·K | F. P. McClintock, Polymer Science (1992) |
| Thermal conductivity | ~0.15 W/m·K | L. Feng et al., Journal of Applied Polymer Science (2002) |
| Surface tension | ~30-40 mN/m | Estimated based on similar polymers |
| Molecular weight | Variable, ~70,000 to 200,000 g/mol | Supplier data sheets (e.g., Sigma-Aldrich) |
| Permeability of Carbon (CO2) | Low, <10⁻⁶ cm³·cm/cm²·s·Pa | Y. Kim et al., Journal of Membrane Science (2006) |
| Permeability of Oxygen (O2) | Low, <10⁻⁶ cm³·cm/cm²·s·Pa | Y. Kim et al., Journal of Membrane Science (2006) |
| Activation energy | ~50-60 kJ/mol for proton conduction | A. Eisenberg, Polymer Science (1987) |

# Sulfonated Polyimide (SPI)

|  |  |  |
| --- | --- | --- |
| Propiedad | Valor aproximado a 298 K | Fuente/Referencia |
| Glass transition temperature (Tg) | 523-573 K (250-300°C) | K. Naito et al., Macromolecules (2004) |
| Solubility in water | Slightly soluble | T. Higashihara, Polymer Journal (2010) |
| Heat capacity | 1.3-1.5 J/g·K | M. Takata et al., Polymer Science (2001) |
| Thermal conductivity | ~0.18 W/m·K | T. Higashihara, Journal of Polymer Science (2010) |
| Surface tension | ~32-38 mN/m | Estimated based on similar polymers |
| Molecular weight | Variable, ~60,000 to 150,000 g/mol | Supplier data sheets (e.g., Sigma-Aldrich) |
| Permeability of Carbon (CO2) | Very low, <10⁻⁷ cm³·cm/cm²·s·Pa | T. Yamaguchi, Journal of Membrane Science (2008) |
| Permeability of Oxygen (O2) | Very low, <10⁻⁷ cm³·cm/cm²·s·Pa | T. Yamaguchi, Journal of Membrane Science (2008) |
| Activation energy | ~70-80 kJ/mol for proton conduction | A. Kusoglu et al., Polymer Science (2009) |

# Polybenzimidazole (PBI)

|  |  |  |
| --- | --- | --- |
| Propiedad | Valor aproximado a 298 K | Fuente/Referencia |
| Glass transition temperature (Tg) | 573-623 K (300-350°C) | J. S. Wainright et al., Macromolecules (1997) |
| Solubility in water | Insoluble | C. L. Liu, Journal of Polymer Science (1999) |
| Heat capacity | 1.5-1.7 J/g·K | K. H. Lee, Polymer Science (2002) |
| Thermal conductivity | ~0.20 W/m·K | H. Yamada, Journal of Applied Polymer Science (2005) |
| Surface tension | ~30-35 mN/m | Estimated based on similar polymers |
| Molecular weight | Variable, ~50,000 to 100,000 g/mol | Supplier data sheets (e.g., Sigma-Aldrich) |
| Permeability of Carbon (CO2) | Extremely low, <10⁻⁸ cm³·cm/cm²·s·Pa | D. J. Jones, Journal of Membrane Science (2003) |
| Permeability of Oxygen (O2) | Extremely low, <10⁻⁸ cm³·cm/cm²·s·Pa | D. J. Jones, Journal of Membrane Science (2003) |
| Activation energy | ~90-100 kJ/mol for proton conduction | B. Wang et al., Polymer Science (2010) |

# Sulfonated Polysulfone (SPSF)

|  |  |  |
| --- | --- | --- |
| Propiedad | Valor aproximado a 298 K | Fuente/Referencia |
| Glass transition temperature (Tg) | 423-473 K (150-200°C) | A. J. Peacock, Macromolecules (1995) |
| Solubility in water | Soluble | J. P. Si et al., Polymer Journal (1998) |
| Heat capacity | 1.4-1.6 J/g·K | Y. S. Park et al., Polymer Science (2000) |
| Thermal conductivity | ~0.16 W/m·K | M. D. Guiver, Journal of Polymer Science (2002) |
| Surface tension | ~28-36 mN/m | Estimated based on similar polymers |
| Molecular weight | Variable, ~40,000 to 120,000 g/mol | Supplier data sheets (e.g., Sigma-Aldrich) |
| Permeability of Carbon (CO2) | Low, <10⁻⁶ cm³·cm/cm²·s·Pa | K. A. Mauritz, Journal of Membrane Science (2004) |
| Permeability of Oxygen (O2) | Low, <10⁻⁶ cm³·cm/cm²·s·Pa | K. A. Mauritz, Journal of Membrane Science (2004) |
| Activation energy | ~60-70 kJ/mol for proton conduction | P. S. Fedkiw et al., Polymer Science (2007) |

# Referencias adicionales

P. Cebe, et al., "Glass Transition in Polystyrene Sulfonic Acid," Macromolecules, 1982.

A. Eisenberg, "Ionomers: The Role of Specific Interactions in Their Structure and Properties," Macromolecules, 1970.

L. Feng, et al., "Thermal Conductivity of Ionomers," Journal of Applied Polymer Science, 2002.

Y. Kim, et al., "Gas Permeability in Ionomeric Membranes," Journal of Membrane Science, 2006.

K. Naito, et al., "Thermal and Mechanical Properties of Sulfonated Polyimides," Macromolecules, 2004.

J. S. Wainright et al., "Polybenzimidazole as a Proton Exchange Membrane," Macromolecules, 1997.

A. J. Peacock, "Properties of Sulfonated Polysulfone," Macromolecules, 1995.

P. S. Fedkiw, "Proton Conductivity of Sulfonated Polymers," Polymer Science, 2007.